Secvest IP FUAA10010 / FUAA10011

History


Version: V2.3.4
Release Date: 26.04.2012
Filename: sh3ab_2.3.4.iso (Secvest_IP_2.3.4.zip)

Important information for this software version:

- Please delete you browser cache after successull firmware upgrade to ensure new user interface is shown correctly
- Please download latest user manual from ABUS Security-Center homeage which includes description for lastest fimware features (DE / UK Version, remaininglanguages will be avilable soon). 


Changes:

1. Polish system language added
2. Added event trigger time for outputs (radio and wired) with following values: always, 1/5/10/15/30/45 and 60 seconds
3. Combination of each event type in output settings is now possible to setup (manual event limitation removed)
4. Added scheduler function for switching outputs and automated arm- and disarming of alarm center
5. Live snapshot function in overview mode for FUAA10010 removed (not supported)
6. E-Mail delivery on entry alarm will now processed after specified entry time setting
7. Entry alarm time settigns on vZones are no longer overwritten



Version: V2.0.5
Release Date: 08.02.2012
Filename: sh3ab_2.0.5.iso (Secvest_IP_2.0.5.zip)

Changes:

1. Detection for offline devices within virtual zones when do SET and PartSET
2. Integration of push notification for Apple mobile devices (Secvest IP App 2.0 required)
3. Setting of automatic data on connected PIR network cameras improved. The setting “verification” will no longer overwritten
4. No alarm e-mail will send out on system SET by remote control if a zone remains open. 



Version: V2.0.0
Release Date: 11.11.2011
Filename: sh3ab_0.7.7.iso (Secvest_IP_2.0.0.zip)

Changes:


1. CASA10010 IP-Alarm module supported (Firmware 2.1 build 110726 required)
2. Detection for offline devices within virtual zones
3. New zone status “yellow” in overview page to indicate offline devices
4. SET command is blocked in case of offline devices detected
5. Input of invalid IP addresses and ports for setup of virtual zones are blocked
6. Configuration of PIR camera sensor setting “internal” and “external” directly in vChannel configuration page
7. Individual alarm events including reference of triggered zone displayed within event log


Version: V1.5.0
Release Date: 01.02.2011
Filename: sh3ab_1.0.5.iso (Secvest_IP_1.5.0.zip)

Changes:

1. SET/UNSET appears only once per command within event log.
2. Solved problem by SET via web interface, followed by SET command via RF-Key
3. E-Mail recipients still shown in rules section even they are deleted already
4. Secondary user couldn't connect by iPhone APP (1.02)
5. Manual event setting for radio output 1/2 doesn't allow event triggered setting at the same time to avoid miss-configurations
6. Wireless outdoor siren is now deactivated in battery mode when UNSET
7. Detectors / Zones showing a battery fault couldn't be bypassed
8. An entry event now keeps alarm status even when detector is closed again whithin delay time without UNSET by user.
9. Triggering transistor outputs works also with silent alarm
10. Triggering transistor outputs works also when settings changed from silent to normal without restart.
11. Support for special characters in password phrases. Un-allowed characters will be blocked already when setup the user password.
12. Custom System name now appears in e-mail subject 
13. System name is shown in SecvestIP web interface
14. E-mail test button
15. Support for custom e-mail subjects, individually for every event type.



Version: V0.7.7
Release Date: 14.01.2011
Filename: sh3ab_2.05.iso (Secvest_IP_0.7.7.zip)

Initial Firmware