Firmware compatible to: HDCC90001, HDCC90011, HDCC90021


Version:V3.6.23_221123
Release Date: 29.11.2022
Filename: HDCC900x1_V3.6.23_221123.dav

FIX: TLS SSL Update for email function

Version:V3.6.23_201218
Release Date: 14.01.2021
Filename: HDCC900x1_V3.6.23_201218.dav

Changes: 

- Fixed issues with IPCS84xxx ABUS speeddome series (Presets, Park Position and Streaming)
- Fixed ABUS Server issue:  After reboot device needs some time to connect to ABUS Server service. 


History:


Version:V3.6.22_191231
Release Date: 12.11.2020
Filename: HDCC900x1_V3.6.22

Changes: 

1. FIX: ABUS Server function, input of username and password not possilbe and correction of server adress

It is recommended to reset the DVR to factory defaults after upgrading firmware.
After upgrade please delete your browser cache!






Version: V3.6.21 Build 190707
Release Date: 07.09.2019
File name: HDCC900x1_V3.6.21.dav 

Fix:
1. ABUS Link Station function added


Version: V3.6.20 Build190411
Release Date: 11.04.2019
File name: HDCC900x1_V3.6.20.dav 

Fix: 

1. USB keyboard TVAC26010 fix with ABUS CMS Software
2. Stream parameter of 3MPx TVI series cameras can be adjusted and saved correctly. 


Version: V3.6.20 Build180605
Release Date: 04.06.2018
File name: HDCC900x1_V3.6.20.cap 


1. Support CVI (max.1080p), AHD, CVBS (PAL/NTSC) and TVI (HDCC90001 max.5MPx, HDCC90011/HDCC90021: max. 8MPx) signals on the BNC inputs.
2. Supports new camera modells HDCC68550, HDCC78550 [NOTE: HDCC90001 does not support 4K cameras]
3. Supports ONVIF cameras. [NOTE: Only 2 additional IP cameras supported, max. resouliton 6MPx]
4. Supports ABUS IP cameras (IPCB42501, IPCB42551, IPCB62500, IPCB72501)  [NOTE: Only 2 additional IP cameras supported, max. resouliton 6MPx]
5. Performance improvements

It is recommended to reset the DVR to factory defaults after upgrading firmware.

History:

Initial firmware:

V3.5.20_build171115  and V3.5.20_build180313



