Version:
Base station 1.0.0.12
Camera firmware 0.0.36.0
Wifi version 0.5.2.0


Changes:
Default-language for voice prompt changed back to german

Firmware update:
1. now disconnect the base station from the power supply.

2. copy the following files to the SD card:
rootfs SMH T1R.img
rootfs SMH T1R.md5
dsp SAPP TAS.bin
dsp RVDP TAS. bin
wifi RVDP TAS.bin
wifi SAPP TAS.bin

3.plug the base station with inserted SD card back into the socket.

The LED will start flashing red after about 20 seconds after initially being solid blue,
This is to confirm that the firmware update has been started successfully.

During the update process, the power supply to the base station must not be disconnected!

The process takes about 120 seconds and is completed as soon as:
a) For actively installed systems:... the voice command " Successfully connected to the network " is played. (With activated voice command setting)
b) For reset or non-configured systems: the voice command "Ready to connect to the network" is heard. (If the voice command setting is activated)

Start firmware update camera:

1.turn on the camera by pressing the power on icon once briefly. 2.

2. place the camera in the immediate vicinity of the base station so that there are no disconnections!
interruptions in the connection! Place the camera with the lens on a flat surface. 3.

Press the pairing button on the base station once.

The LED on the base station will start flashing red to confirm that the firmware update has been
update has been successfully started. The LED on the front of the camera will briefly flash blue.
The process takes approx. 300 seconds and is completed as soon as the voice command "Firmware update
Update successfully completed" is played.

If the voice command "Firmware update failed, please try again" is played,
repeat the process by pressing the "Pairing Button" once. 
If the update still fails, please contact the customer support.

4.Now open the app and go to the advanced settings.
Under the device information, check if the version has been updated to 1.0.0.12.
Check if the F/W version has been updated to 0.0.36.0 and the Wi-Fi version has been updated to 0.5.2.0 in the camera settings.