Firmware compatible to: PPDF16000

History

Version: 1245
Release date: May 2018
File name: r4_rx_rootfs-cpio_master.squashfs.img , r3_uImage_828x

Changes
•	On the App-Setup the password can now be changed inside the app

Firmware-Update:
1. Copy the two files xxx.img and _828x onto an emtpy microsd-card
2. Insert the microsd card into the monitor
3. Navigate to the Storage settings - systeminformation
4. Click on Upgrade
5. Choose "Receiver Firmware Upgrade" so a checkmark appears besides the line
6. Click on "OK"
You must not disconnect the monitor from the power supply during the firmware update, as this may result in irreparable damage to the device. The update procedure takes about 3 minutes

